**Exhibit C**

**Engineering Specifications for an Overhead Bipolar HVDC Transmission Line**

**Segment    of**

General information

1. Name of Petitioner:

2. Name or Circuit Number of Line:

3. Length of Segment:       miles

4. Segment is located in the following sections, townships, and ranges:

5. Segment in     .

6. Segment will be maintained in accordance with the Iowa Electrical Safety Code and the      Edition of the National Electrical Safety Code.

7. Maximum *Capable of Operating* Voltage:      kVDC Nominal Operating Voltage:      kVDC

nesc rule 232D Vertical overhead clearance requirements

8. Maximum DC Operating Voltage to Ground in Kilovolts: (V) =

9. Maximum Switching Surge Factor: (PU) =

10. Electrical Component of Clearance: (D) =

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Nature of Surface Underneath Lines** | **Table 232-3 Reference Height** | **+** | **Electrical Component of Clearance (D)** | **=** | **Clearance\*** |
| 11. | *Open Ground* | 14 ft. | + |       ft. | = |       ft. |
| 12. | *Roads* | 14 ft. | + |       ft. | = |       ft. |
| 13. | *Railroads* | 25 ft.\*\* | + |       ft. | = |       ft. |
| 14. | *Water* | 12.5 ft. | + |       ft. | = |       ft. |
| 15. | *Water Areas Suitable for Sailboating**(<20 acres)* | 16 ft. | + |       ft. | = |       ft. |
| 16. | *Water Areas Suitable for Sailboating**(20 to 200 acres)* | 24 ft. | + |       ft. | = |       ft. |
| 17. | *Water Areas Suitable for Sailboating**(200 to 2000 acres)* | 30 ft. | + |       ft. | = |       ft. |
| 18. | *Water Areas Suitable for Sailboating**(>2000 acres)* | 36 ft. | + |       ft. | = |       ft. |
|  | \* The Iowa Electrical Safety Code and the applicable edition of the NESC should both be referenced to determine the conditions at which the above clearances apply. |
|  | \*\* 199 IAC 42.6(2)”a” requires the height of a rail car to be 23 feet, 3 feet higher than the NESC, when calculating clearances.. |

ConductorS and insulators

19. Number of Conductors per Bundle:

20. Conductor Code Word:       Size:       MCM Stranding:       Material:

21. Typical Tangent Structure Insulators:

22. Typical Strain Structure Insulators:

|  |  |
| --- | --- |
|  | **Insulator Bell Electrical Characteristics in Accordance with IEC 61325** |
|  |  | DC Withstand Voltage | Dry Lightning Impulse Withstand Voltage | DC SF6 Puncture Withstand Voltage |
|  | Catalog Number | Dry 1 Minute | Wet 1 Minute |
| 23. |       |       kV |       kV |       kV |       kV |
| 24. |       |       kV |       kV |       kV |       kV |

25. Number of Metallic Return Conductors (MRC):

26. MRC(s) Maximum Operating Voltage:       MRC(s) Typical Operating Voltage:

27. MRC(s) Code Word:       Size:       MCM Stranding:       Material:

28. Shield Wire(s):

Typical Tangent Structures

29. Construction Grade: Typical Span:       ft. Maximum Span:       ft.

30. Typical Tangent Structures are:

31. Typical Height After Installation:       ft.

TYPICAL STRUCTURE DRAWING

32. A dimensioned drawing of a typical tangent structure  been attached.

ADDITIONAL DRAWINGS REQUIRED FOR NEW CONSTRUCTION

33. Angle structures be used in this segment of line. A dimensioned drawing of a typical angle structure  been attached.

34. Dead-end structures be used in this segment of line. A dimensioned drawing of a typical dead-end structure been attached.

35. There along this segment of line. Drawings showing the clearance envelope for each grain bin in relation to the proposed line .